**New Flooring Tender – Details**

**Required Works:**

Take up Existing Flooring – Remove all doors as necessary.

Install polysafe flooring including membrane, screed & level as required etc. to below detailed areas

Shave doors and refit

All costs are to include the supply of skips etc. for safe removal of existing floor coverings. All waste products are to be disposed of in a responsible manner and in compliance with current waste regulations.

Please provide full details of product specifications

|  |  |  |  |
| --- | --- | --- | --- |
| **Area**  | **Room(s)** | **Base & Current Flooring** | **Area m2**  |
| Humanities | 1, 2, 3, 4 & Corridors | Solid baseCarpet overlay | 1 = 52.8 2 = 52.83 = 52.84 = 52.8Corridor = 16.4 |
| Drama  | 10 & 11  | Solid base with wooden floorboard overlay | 10 = 62.8411 = 61.02 |
| Science | 7, 8 & Prep Room | Solid base with vinyl tile overlay | 7 = 63.51Prep = 25.758 = 63.84 |
| IT  | 45 | Solid baseCarpet overlay | 46.61 |
| DT / Res Mat | 42, Tech Prep Room | Solid baseNon-slip flooring | Tech Prep Room = 35.13 42 = 154.52 |
| Business  | 29, 30, 31, 32  | Solid base with vinyl tile overlay | 29 = 48.7930 = 49.4631 = 50.0332 = 46.95 |
| Sports  | Changing Rooms & Corridors  | Solid base with ceramic non-slip tile overlay | Boys = 48.52 + 3.00Girls = 48.68 + 2.99 |
| Classroom | 49 | Solid baseWooden Floorboard overlay plus Carpet  | 41.90 |

Please return all quotes to tenders@rlt.education, using "Heys - Flooring" as the subject line. Deadline 12 noon 7th May 2021